    File   Dcp1_anglais.mdf
          IFREMER - FAD calculation Module  -    14/05/04 - 16:25:54          

DESCRIPTION OF THE STRUCTURE
Number of knots
2

Description of the knots
1      0.000      0.000    -10.000          1 1 Type 1 Corps mort
2      0.000      0.000      0.000          1 2 Type 2 Flotteur

Number of elements
1

Description of the elements
1          1          2          1 Elément 1,5 3

NUMERICAL PARAMETERS
Added stiffness (N/m)
1000000.000000

Convergence threshold(N) :
1.000000

Limit of movement at each iteration step (m) :
1.000000

Maximum number of iterations step :
50000

Dynamic : Calculation time step (s) :
0.500000

Dynamic : Time step for writing data on file (s) :
0.500000

Dynamic : Starting time for writing data (s) :
0.000000

Dynamic : Finishing time for calculation and writing data (s) :
10.000000

METEOROLOGICAL AND  ET OCEANIC ENVIRONMENT
Courant
	Current constant
1
	Direction (deg) :
0.000000

	Speed (m/s) :
0.500000

Waves
	Period (s) :
5.000000

	Height (m) :
1.000000

	Direction from X (deg) :
0.000000

Water depth (m) :
10.000000

LISTE OF KNOTS TYPES
Number de Types :     3

	N° of type                  :  1
	Name of type                 :   Type 1 Corps mort
	Masses X,Y,Z (kg)           :   1000.000000 1000.000000 1000.000000
	Added Masses  X,Y,Z (kg)  :   1000.000000 1000.000000 1000.000000
	Lengths X,Y,Z (m)         :   0.500000 0.500000 1.000000
	Drag Coef. X,Y,Z         :   1.200000 1.200000 1.200000
	Extern Forces X,Y,Z (N):   0.000000 0.000000 0.000000
	Movement X,Y,Z           :   1 1 1
	Limits X,Y,Z (m)           :   99.000000 99.000000 99.000000
	Limits directions X,Y,Z      :   0 0 0


	N° of type                  :  2
	Name of type                 :   Type 2 Flotteur
	Masses X,Y,Z (kg)           :   20.000000 20.000000 20.000000
	Added Masses  X,Y,Z (kg)  :   20.000000 20.000000 20.000000
	Lengths X,Y,Z (m)         :   0.403000 0.403000 0.403000
	Drag Coef. X,Y,Z         :   0.604000 0.604000 0.604000
	Extern Forces X,Y,Z (N):   0.000000 0.000000 0.000000
	Movement X,Y,Z           :   0 0 0
	Limits X,Y,Z (m)           :   0.000000 0.000000 0.000000
	Limits directions X,Y,Z      :   0 0 0


	N° of type                  :  3
	Name of type                 :   Type 3 Liaison
	Masses X,Y,Z (kg)           :   0.000000 0.000000 0.000000
	Added Masses  X,Y,Z (kg)  :   0.000000 0.000000 0.000000
	Lengths X,Y,Z (m)         :   0.000000 0.000000 0.000000
	Drag Coef. X,Y,Z         :   0.000000 0.000000 0.000000
	Extern Forces X,Y,Z (N):   0.000000 0.000000 0.000000
	Movement X,Y,Z           :   0 0 0
	Limits X,Y,Z (m)           :   0.000000 0.000000 0.000000
	Limits directions X,Y,Z      :   0 0 0


LISTE OF ELEMENTS TYPES
Number of Types :		1

	N° of type                  :  1
	Name of type                 :  Elément 1
	Elasticity Modulus (pa)                 :  2950000000.000000
	Stiffness in traction (N)        :  1000000.000000
	Stiffness in compression (N)     :  1.000000
	Length at rest (m)       :  25.000000
	N° and name of material       :  12 Polyamide PA
	Diameter (m)      :  0.020000
	Traction/Compression ratio       :  1000000.000000
	Volumic mass(kg/m3)     :  1025.000000
	Hydrodynamic diameter (m) :  0.020000
	Normal Cd                    :  1.200000
	Tangential Cd                :  0.080000
	Number of bars (discretization)            :  5
	Type of knot (discretization)               :  3

